Shows Lane End

Image processing

Follow the Lane

Gives the instruction of Lane position to Robot

Capture image by Sensor

No

Find lane

No

Yes

Obstacle detect

Yes